2017 Lamborghini Huracan LP640-4 Performante

Info
A track oriented variant of the Huracán, called the Performante, was unveiled at the 2017 Geneva Motor Show.

The Performante underwent various exterior changes with the most noticeable being the front and rear bumpers.
Carbon fibre is used for the bumpers and the side skirts. An adjustable carbon fibre rear wing has been added
to increase downforce. The position of the exhaust has also been changed, and is now just a bit above the rear diffuser.
The interior also underwent noticeable changes, now sporting new seats and a new digital speedometer (similar to that of the Aventador SV's speedometer).

The Performante's 5.2-liter V10 has been tuned to have a power output of 471 kW (631 hp; 640 PS) at 8,000 rpm and
601 N⋅m (443 lb⋅ft) of torque at 6,500 rpm. The weight has also decreased by 40 kg (88 lb), courtesy of the forged aluminium
and forged carbon fibre body components (first used in the construction of the Sesto Elemento). All the new aero components on the car
have active aerodynamic capability and help keep the car stable at high speeds. The Performante is capable of accelerating from
0–100 km/h (0–62 mph) in 2.9 seconds and has a theoretical top speed of 351 km/h (218 mph).

The car has been stiffened by 10% with new springs, roll bars, and radial axial arm bushings. The magnetorheological
suspension has been reworked to give a driver a serious track experience. The Lamborghini Dynamic Steering has been re-calibrated.
The Performante utilises Lamborghini's new ALA (Aerodinamica Lamborghini Attiva) system, which is said to be 80% lighter than regular sports
car hydraulic systems. According to Lamborghini, ALA is also said to provide 750% more downforce than the standard Huracán.
The price of the car is set at US$274,390.

Performance
Power: 630.7 hp (470 kW)
Torque: 599.5 nM (443 lb-ft)
Top Speed: 325 km/h (201.5 mph)
Weight: 1382 kg (3047 lbs)

Special Colors
116,195,101			# 127 jvt verde mantis			green
247,127,33			# 128 jvt arancio borealis		orange

Carcols: 128,36, 1,61, 15,61, 6,36, 53,36, 0,36, 3,61, 127,36
Handling: 1382.0    3047.0   1.48    0.0 0.0 -0.15  75  0.65 1.0 0.47 	5 355.0 63.1 90.0 4 P 	9.1  0.62 0 30.0   1.0  0.16  0.0  0.25 -0.115 0.4  0.27		0.16 0.61 274390 	c0112004			C02200		0  1	0
Vehicles: 506, 	supergt, 	supergt, 	car, 		SUPERGT, 	SUPERGT, 	null,	executive, 	5, 	0,	0,		-1, 0.76, 0.76,		0